*Heading
*Preprint, echo=NO, model=NO, history=NO, contact=NO
*Part, name=Part-1
*Node
*Element, type=C3D8H
*Nset, nset=_PickedSet2, internal, generate
*Elset, elset=_PickedSet2, internal
*Solid Section, elset=_PickedSet2, material=user
*End Part
*Assembly, name=Assembly
*Instance, name=Part-1-1, part=Part-1
*End Instance
*Nset, nset=Set-1, instance=Part-1-1
*Nset, nset=Set-2, instance=Part-1-1
*Nset, nset=_PickedSet4, internal, instance=Part-1-1
*Elset, elset=_PickedSet4, internal, instance=Part-1-1
*Nset, nset=_PickedSet5, internal, instance=Part-1-1, generate
*Elset, elset=_PickedSet5, internal, instance=Part-1-1
*Nset, nset=_PickedSet6, internal, instance=Part-1-1, generate
*Elset, elset=_PickedSet6, internal, instance=Part-1-1
*Nset, nset=_PickedSet7, internal, instance=Part-1-1
*Elset, elset=_PickedSet7, internal, instance=Part-1-1
*End Assembly
*Amplitude, name=Amp-1, time=TOTAL TIME
             0.,              0.,              1.,              1.,              2.,              0.
** ----------------------------------------------------------------
** User Material Interface
**
*Material, name=user
*Depvar
*User Material, constants=5
** ----------------------------------------------------------------
*Step, name=Step-1, nlgeom=YES, inc=10000
*Static, direct
0.01, 2.,
*Boundary
_PickedSet4, 3, 3
*Boundary
_PickedSet5, 1, 1
*Boundary
_PickedSet6, 2, 2
*Boundary, amplitude=Amp-1
_PickedSet7, 3, 3, 5.
*Restart, write, frequency=0
*Print, solve=NO
*Output, field, variable=PRESELECT
*Output, history
*Node Output, nset=Set-1
U3,
*Node Output, nset=Set-2
RF3,
*Output, history, variable=PRESELECT
*End Step